|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Hazard | Existing control measures | Harm (1-5) | Likelihood (1-5) | Risk (1-5) | Further controls |
| Electric shock | Annual PAT test | 5 | 1 | 1 | Keep users away from electrical cables |
| User behaviour, overcrowding or tipping over | Users limited in numbers to the recommended manufacturer's amount shown on the front of each inflatable | 2 | 1 | 1 | Supervision at all times at both ends of the inflatable |
| Over enthusiastic participants | Adult supervision at all times | 2 | 1 | 1 | None |
| Adverse weather conditions | Item to be switched off in heavy rain and/or high winds and not to be used | Dependent upon the weather | Dependent upon the weather | Dependent upon the weather | None |
| Danger of unnecessary injury | No one with a history of neck, back, heart or other medical conditions, pregnant women or anyone under the effects of alcohol or drugs should be using the equipment | 5 | 1 | 5 | None |
| Danger of fire | No smoking, bbq's, fireworks or candles allowed near the inflatable | 5 | 1 | 1 | None |
| Emergency | In the event that someone is seriously injured, do not move the individual, leave the inflatable switched on and dial 999 | 5 | 1 | 1 | None |
| Larger participants colliding with smaller participants | Adult supervision at all times | 1 | 1 | 1 | Participants put into groups based on size and age |
| Choking | No food or drink taken onto the inflatable | 1 | 4 | 4 | None |
| Drowning | Do not leave anyone unattended on the waterslide | 5 | 4 | 4 | Constant supervision at both ends of the inflatable |
| Injury from 3rd party items | All shoes, glasses, jewellery, badges etc to be removed before using the inflatable | 5 | 1 | 1 | Supervision – do not allow any items to be taken on the inflatable |
| Danger from falling from height | Adult supervision at all times | 1 | 3 | 3 | Ensure no one is climbing on the walls of the inflatable |
| User behaviour/ collision | Adult supervision at all times | 1 | 3 | 3 | Ensure only one user at a time on the slide element to reduce collision risk |
| Trip hazard from anchor points or electrical cable | All anchor points used as per manufacturer's instructions and electrical cable to be run behind the inflatable away from participants | 1 | 1 | 1 | None |
| Any other localised risks:  1.  2.  3. |  |  |  |  |  |

|  |  |  |
| --- | --- | --- |
| Risk Assessment carried out by: | Date: | Any other action required |
|  |  |  |